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Purpose:  
The purpose of the policy is to set out terms and conditions for gravelling approaches within the Rural Municipality (RM) of Oakview, including;
Rural Gravel roads
Urban and LUD Driveways and Approaches.
Addition of Culverts in Driveways and Approaches.
            Covering of Access Surfaces with Material other than Gravel.
Approved approaches guidelines
Policy:

 Rural Gravel Roads

It is the policy of the Rural Municipality of Oakview not to place, supply, or maintain gravel on Rural Gravel Road private approaches to home or farmyard sites for landowners / ratepayers. It will be the responsibility of the landowner / ratepayer to maintain, supply and place gravel on their approaches if deemed necessary.

Urban and LUD Driveways and Approaches


It is the policy of the RM of Oakview not to place, supply or maintain gravel on Urban or Private driveways located within the boundaries of Rapid City, Oak River LUD’s, including the urban areas of Basswood and Cardale.
  
It will be the responsibility of the landowner / ratepayer to supply, place, or maintain gravel on their approaches if deemed necessary. This includes driveways 



that cross over median access road allowances belonging to the RM of Oakview. Access driveways and lanes under the RM or LUD’s authority require written application to create access to lots that encroach onto RM property before any new development can commence.

Addition of Culverts to Driveways and Approaches

Should the additional application for a drainage culvert be required within the access, it must comply with the Provincial or Municipal drainage plan requirements of the area and not cause any adverse effects to RM infrastructure or neighboring properties.

The initial culvert will be supplied at cost to the applicant and maintained by the RM or LUD at no cost, following successful application of approval granted, by The Province, RM or LUD. The installation of the culvert will be at the landowners / rate payer’s full cost.

In the event of the property owner / rate payer causing damage to the culvert structure, the full financial cost will be borne by the registered property lot or parcel landowner / ratepayer.

Should culvert repair, maintenance or renewal of the culvert be required, due to RM or LUD operative damage, inclusive of natural aging, this will be at the full cost of the RM or LUD.

Covering of Access Surfaces with Material other than Gravel.

If a landowner or rate payer requests road approaches, driveways or lanes to be made or covered with any material other than road quality gravel, a written application to the RM or LUD will be needed.

Following approval of application, the full cost of all future repair maintenance and renewal of the culvert, driveway, approach or laneway will be borne by the property lot or parcel owner.


Adverse Weather Conditions affecting Driveways and Approaches.

In the event of damage caused by a flood adverse weather event, the RM and LUD’s will endeavor to inform landowners / rate payers of the due process of Disaster Financial Assistance (DFA) claim procedure if applicable. The RM and LUD’s are not responsible for any damages caused by adverse weather conditions.



                   

 Approved approaches should be within the following guidelines;
· Residential (within Town Limits) - minimum of 20 feet and maximum of 30 feet
· Residential (Ag) – minimum 30 feet and maximum of 40 feet
· Agricultural – minimum of 40 feet and maximum of 60 feet
· Commercial – minimum of 30 feet and maximum of 60 feet
Exceptions to the above may be made by Council in circumstances that they may   deem warranted.


SCHEDULE “A”

Standards and Specifications

1. Approaches must be constructed to Oakview specifications.  Municipality to be notified prior to commencement of work.

1. Due consideration for appropriate setback distances from intersections and obstructions causing a visibility hazard must be given. 

1. Minimum width of clearing will be determined by the Municipality.

1. No brush piles and /or debris are to be left on adjacent land upon completion of construction.  All brush piles and /or debris are to be disposed of.

1. Permit from Manitoba Water Stewardship must be obtained if a culvert is to be replaced or added.

1. Culvert if required must be new and be sized appropriately as per the permit.

1. 4:1 grade slope must be maintained. 

1. Approach base and aggregate materials used must be suitable for approach 
construction.

1. All Utility line locates required where applicable.

1. Survey may be required with costs to be borne by ratepayer.

1. Approved approaches should be within the width guidelines listed on page 1.
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